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NAME：KX-9762 High Speed Automatic Coil Winding Machine
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SPECIFICATION:
	Spindles
	2
	Spread Motor
	4-Phase stepping Motor

	Wire diameter
	0.02-0.8mm
	Max Speed
	6000rpm

	Spread Pitch
	0-9.999mm
	Memory
	999 Sequences

	Spread Width
	100mm（Max）
	Power Source
	AC 220V/110V±10%,50/60MHZ

	Winding Width
	150mm（Max）
	Weight
	50×67×10

	Main Motor
	1/2HP DC Motor
	Dimension
	50


FEATURES:

High Speed Automatic Coil Winding Machine has microprocessor design ,easy for program-setting handing.

input the ‘Start Point’parameter by number key or teachable function ,and display the position of spreading head on the panel

The wire of High Speed Automatic Coil Winding Machine runs though the nozzle of spreading head to arrange in order better

Multiple spindles synchronal winding for highest efficiency

High Speed Automatic Coil Winding Machine has more convenience by using foot-switch

ADVANTAGES:

Adopt multi - winding head, four different diameters can be installed at the same time.
Single High Speed Automatic Coil Winding Machine can finish winding and insulation, acetic acid tape function.
You can change the program to achieve functionality as needed.
The position of the spool can be adjust with the teaching function, which can assist the setting of the winding point and width position.
0~999 group data is easy to set, with powerful DC motor and precision stepper motor, it can easily set forward reverse, cross slot and flow tight winding work.

APPLICATION:
High Speed Automatic Coil Winding Machines are used for winding the small EI transformers, signal transformers, inductors, filter choke coil, relays, current contactors, valve coils, solenoid coils, telecom bobbin transformers. It can complete the coils without any one operator in fully automatically.

PRACTICAL APPLICATION :

Training for Customers to Operate KX-9762 High Speed Automatic Coil Winding Machine

1.All service engineers with 10 years of experience have received special technical training, including specialized expertise in the KX-9762 High Speed Automatic Coil Winding Machine, enabling them to effectively handle various breakdown issues specific to this high-performance equipment, such as automatic feeding system malfunctions, high-speed spindle instability, or sensor errors in the automated winding sequence.

2.We guide users to accurately operate and maintain the KX-9762 High Speed Automatic Coil Winding Machine—with focused attention to its automated parameter setup (including winding speed, turn count, and wire tension), calibration of the automatic wire threading mechanism, and maintenance of critical components like the high-frequency motor and precision control sensors—while providing free consultation about the production process technology related to electronic coil manufacturing, including optimal strategies for balancing speed, accuracy, and coil quality in high-volume production.

3.To ensure the KX-9762 High Speed Automatic Coil Winding Machine operates normally, we conduct dedicated training on its automated operational protocols, troubleshooting of high-speed performance issues, and preventive maintenance of wear-prone components through English manuals, model-specific instructional videos, and real-time online guidance—all tailored to the unique high-speed and automated features of this advanced coil winding equipment.

PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for High Speed Automatic Coil Winding Machine , Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale High Speed Automatic Coil Winding Machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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OPTIONAL ACCESSORIES

	NO.
	Item/Specification
	QUANTITY
	UNIT

	1 
	controller
	1
	PIECE

	2 
	winding motor
	1
	PIECE

	3 
	Spread motor
	1
	PIECE

	4 
	optical fiber sensor
	1
	PIECE

	5 
	B2-2.0 Inches shuttle
	1
	PIECE

	6 
	4 inches and 6 inches shuttle                                                           (base on machine model)
	1
	PIECE

	7 
	shuttle guide wheel
	1
	PIECE

	8 
	fixture head
	1
	PIECE

	9 
	green round belt                                                                                 (can send one free in orange)
	1
	M

	10 
	gear shape belt
	1
	Belt


FACTORY:

We, KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD., have been experts in winding machine lines for 28 years, with our advanced product portfolio featuring high-performance equipment like the KX-9762 High Speed Automatic Coil Winding Machine—a cutting-edge system engineered for rapid, automated coil production, embodying our technical innovation in high-efficiency manufacturing solutions for electronic components.

Our KIOXIA LIGHT RING brand holds authoritative certifications and recognitions, including ISO9001:2015, CE approvals, multiple machine patents (encompassing key innovations in high-speed automation technology for models like the KX-9762 High Speed Automatic Coil Winding Machine), and the official designation of "high-tech enterprise" by the government. These credentials validate the reliability, speed, and precision of our entire product range, reinforcing our commitment to delivering superior winding solutions that meet the demanding requirements of high-volume coil manufacturing.
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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

